 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 1 of 4**

**Building Name:**  **St. Rita of Cascia**

**Building Address:**  **770 W. Old Indian Trail- Aurora, Illinois 60506**

**Name of Person Completing Report:**

**Title:** **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| *~~01~~* | *~~Linoleum~~* | *~~Restrooms by Gym~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| *~~02~~* | *~~1’x1’ Ceiling Tile- Pinhole~~* | *~~Basement & Hallway~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| *~~03~~* | *~~Plaster Ceilings & Walls- Sandy Finish~~* *~~(See HA #SPB)~~* | *~~Basement & Lobby Area~~* | *~~N/A~~* | *~~N/A~~* |  | ***Material Analyzed to be NON-ACM by True North in 2014*** |
| *~~04~~* | *~~1’x1’ Ceiling Tile- Grooved w/Pinholes~~* | *~~Telephone Booth & Office~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| *~~05~~* | *~~2’x4’ Ceiling Tile- Grooved w/Pinholes~~*  | *~~Library~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| *~~06~~* | *~~Fiberglass Ceiling Tile~~* | *~~7th & 8th Grade Classrooms~~* | *~~N/A~~* | *~~N/A~~* |  | Assumed to be ***Fiberglass*** in ***1988*** |
| *~~07~~* | *~~Gypsum Wall Board~~* | *~~Pipe Chase, Hallway to Gym, Storage to Gym~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| *~~08~~* | *~~2’x4’ Ceiling Tile- Rough~~* | *~~Hallway To Gym~~* | *~~N/A~~* | *~~N/A~~* |  | Material analyzed to be ***NON-ACM*** in ***1988*** |
| **09** | **Boiler & Boiler Flue Insulation** | **Boiler Room** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M*** |
| **10** | **Pipe Insulation** | **Boiler Room** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M*** |
| **11** | **Pipe Fittings on Non-ACM Pipe Insulation** | **Throughout** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M*** |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.

 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 2 of 4**

**Building Name:**  **St. Rita of Cascia**

**Building Address:**  **770 W. Old Indian Trail- Aurora, Illinois 60506**

**Name of Person Completing Report:**

**Title:** **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| *~~12~~* | *~~9”x 9” Floor Tile~~* | *~~Throughout Building~~* | *~~N/A~~* | *~~N/A~~* |  | Material ***Removed/Abated*** in ***3*** ***Stages***… ***1990***, ***July 2002***, ***June/July 2004*** |
| *~~13~~* | *~~9”x 9” Floor Tile Mastic- Associated w/HA #12~~* | *~~Throughout Building~~* | *~~N/A~~* | *~~N/A~~* |  | Material ***Removed/Abated*** in ***3*** ***Stages***… ***1990***, ***July 2002***, ***June/July 2004*** |
| *~~14~~* | *~~Acoustical Ceiling Plaster~~* | *~~Church~~* | *~~N/A~~* | *~~N/A~~* |  | Material ***Removed/Abated*** in ***1990*** |
| **15** | **Epoxy Flooring Material** | **Locker Room** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| *~~SPA~~* | *~~Plaster- Smooth Finish~~* | *~~Throughout Building~~* | *~~N/A~~* | *~~N/A~~* |  | ***Material Analyzed to be NON-ACM by True North in 2014*** |
| *~~SPB~~* | *~~Plaster- Sandy Finish~~* | *~~Basement & Lobby Area, Gym Hallway~~* | *~~HA #03~~* | *~~HA #03~~* |  | ***Material Analyzed to be NON-ACM by True North in 2014*** |
| **MDA** | **Drywall W/Compound & Tape** | **Library & Computer Room** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFA** | **12”x 12” Floor Tile/Mastic- Beige w/Tan & Brown Flecks** | **Basement Cafeteria** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFB** | **12”x 12” Floor Tile/Mastic- Beige w/ Aqua, Green & Orange Flecks** | **Principal’s & Nurses Office** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFC** | **12”x 12” Floor Tile/Mastic- Dark And Light Aqua Flecks** | **Classrooms 1S to 4S & 5W to 8W** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFD** | **12”x 12” Floor Tile/Mastic- Dark Gray & Beige Flecks** | **Hallway & Faculty Lounge** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.

 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 3 of 4**

**Building Name:**  **St. Rita of Cascia**

**Building Address:**  **770 W. Old Indian Trail- Aurora, Illinois 60506**

**Name of Person Completing Report:**

**Title:** **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| **MFE** | **12”x 12” Floor Tile/Mastic- Gray & Beige Flecks** | **1st Floor-Front Workrooms & Storage, 2nd Floor- Computer Room** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFF** | **12”x 12” Floor Tile Mastic- Beige & Tan Squares Pattern** | **Gym, Office/Storage** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFG** | **Terrazzo** | **Basement- Stairs, Woman’s Rm, Kitchen 1st Floor- Hallway, Bathroom**  | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFH** | **1” Ceramic Tile/Grout- Gray** | **1st Floor North Boy’s Bathroom** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MFI** | **12”x 12” Floor Tile/Mastic- Brown w/Tan & Beige Flecks** | **Classrooms 1N to 4N & 6E to 8E, Bookroom/Storage, Teacher’s Lounge** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MBA** | **Vinyl Wall Base/ Mastic- Gray** | **Hallway, Storage Rooms** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| *~~MCA~~* | *~~2’x2’ Lay-In Ceiling Tile~~* | *~~Front Storage Rooms~~* | *~~N/A~~* | *~~N/A~~* |  | ***Material Analyzed NON-ACM by True North in 2014*** |
| *~~MCB~~* | *~~2’x4’ Lay-In Ceiling Tile- Small Fissures w/Pinholes~~* | *~~Library~~* | *~~N/A~~* | *~~N/A~~* |  | ***Material Analyzed NON-ACM by True North in 2014*** |
| *~~MCC~~* | *~~2’x4’ Lay-In Ceiling Tile- Rough w/ Pinholes~~* | *~~Hallway to Gym~~* | *~~N/A~~* | *~~N/A~~* |  | ***Material Analyzed NON-ACM by True North in 2014*** |
| **MBB** | **Vinyl Wall Base/ Mastic- Blue** | **Library** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MBC** | **Vinyl Wall Base/ Mastic- Black** | **Hallway to Gym, Gym Office, Faculty Lounge** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.

 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 4 of 4**

**Building Name:**  **St. Rita of Cascia**

**Building Address:**  **770 W. Old Indian Trail- Aurora, Illinois 60506**

**Name of Person Completing Report:**

**Title:** **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| **MMA** | **Fire Doors** | **Basement & 2nd Floor** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MMB** | **Exterior Window Caulking** | **Exterior- Sanctuary Windows** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2011*** |
| **MCD** | **Ceiling Tile/Insulation** | **8W,7W,8E,7E** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by True North in 2014*** |
| **MFJ** | **Sheet Flooring- Tan w/Multi Colored Specks** | **6W,7E** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by True North in 2014*** |
| **MFK** | **Wood Pergo Flooring** | **Gym** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by True North in 2020*** |
| **MMC** | **HVAC Vibration Dampener** | **Gym Storage Room- 2nd Floor** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by True North in 2020*** |
| **MCE** | **2’x2’ Lay-in Ceiling Tile- Smooth Pinhole** | **Basement Cafeteria** | **ND** | **ND** |  | **ASSUMED- Preventive Measures… Continue O&M*****Material Identified by True North in 2020*** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.