 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 1 of 3**

**Building Name: St. Anne School**

**Building Address:**  **1112 N. Brinton Avenue Dixon, Illinois 61021**

**Name of Person Completing Report:**

**Title:**  **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| **01** | **9”x9” Floor Tile/Mastic- Brown, Pink & Tan Speckles** | **Cafeteria, Supply Room, Classrooms 107, 108, West Hallway** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M- Mastic is ASSUMED*** |
| **02** | **9”x9” Floor Tile/Mastic- Brown w/Beige Streaks** | **100,102,103, 104, Kitchen, Copy Rm, Library, Offices, Faculty Bath, Storage, Church** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M- Mastic is ASSUMED*** |
| *~~03~~* | *~~Pipe Insulation~~* | *~~Throughout Building~~* | *~~N/A~~* | *~~N/A~~* |  | Material Analyzed to be ***NON-ACM*** in ***1988*** |
| **04** | **Pipe Fitting Insulation** | **Throughout Building Including Boiler Room & Pipe Tunnels** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M- Abated from Boiler Room 6/2015*** |
| *~~05~~* | *~~Boiler Breeching~~* | *~~Boiler Room~~* | *~~N/A~~* | *~~N/A~~* |  | ***Preventive Measures… Continue O&M- Abated from Boiler Room 6/2015*** |
| *~~06~~* | *~~Window Panels~~* | *~~Throughout Building~~* | *~~N/A~~* | *~~N/A~~* |  | Material Analyzed to be ***NON-ACM*** in ***1988*** |
| **07** | **Linoleum/Mastic- Brown & White Patterned** | **NW Mobile Classroom Building- NE Doorway** | **ND** | **ND** |  | ***Preventive Measures… Continue O&M- Mastic is ASSUMED*** |
| *~~08~~* | *~~Fiberboard Ceiling~~* | *~~Annex~~* | *~~N/A~~* | *~~N/A~~* |  | Material Analyzed to be ***NON-ACM*** in ***1988*** |
| *~~09~~* | *~~Fiberboard “Swamp Grass”~~* | *~~Throughout School~~* | *~~N/A~~* | *~~N/A~~* |  | Material Analyzed to be ***NON-ACM*** in ***1988*** |
| *~~10~~* | *~~9”x9” Floor Tile Mastic~~* | *~~N/A~~* | *~~N/A~~* | *~~N/A~~* |  | ***HA# 10 has been Eliminated and is now Included w/Individual Associated Tiles*** |
| *~~11~~* | *~~Linoleum Mastic~~* | *~~N/A~~* | *~~N/A~~* | *~~N/A~~* |  | ***HA# 11 has been Eliminated and is now Included w/Individual Associated Linoleum- See HA# 07*** |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.

 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 2 of 3**

**Building Name: St. Anne School**

**Building Address:**  **1112 N. Brinton Avenue Dixon, Illinois 61021**

**Name of Person Completing Report:**

**Title:**  **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| *~~12 &~~**~~13~~* | *~~Vinyl Base (HA# 12) & Vinyl Mastic (HA# 13)~~* | *~~N/A~~* | *~~N/A~~* | *~~N/A~~* |  | ***HA#’ s 12 & 13 Descriptions have been Eliminated and are now Included Elsewhere*** |
| **14** | **Drywall w/Compound & Tape** | **Main Office & Library** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **15** | **12”x12” Floor Tile/Mastic- White** | **South Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **16** | **12”x12” Floor Tile/Mastic- White** | **North Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **17** | **Drywall w/Compound & Tape** | **South Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **18** | **Drywall w/Compound & Tape** | **North Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **19** | **Textured Ceiling Paint** | **South Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **20** | **Textured Ceiling Paint** | **North Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M*** |
| **MFA** | **Terrazzo- Brown, Green, Black & Gray Stone Pattern** | **Foyer, Boy’s & Girl’s Bathrooms** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MFB** | **Linoleum- Gray, Beige & Tan** | **Front General Ministry Office** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MDA** | **Drywall w/Compound & Tape** | **Front General Ministry Office** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.

 **SIX MONTH ASBESTOS PERIODIC SURVEILLANCE REPORT Page 3 of 3**

**Building Name: St. Anne School**

**Building Address:**  **1112 N. Brinton Avenue Dixon, Illinois 61021**

**Name of Person Completing Report:**

**Title:**  **Date:**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **HA#** |  **Material Description** | **Locations of material** | **Previous****Condition** **\*\*\*** |  **Current****Condition** **\*\*\***  | **Photo****#** | **Comments** |
| **MDB** | **Drywall w/Compound & Tape** | **NW Mobile Classroom Building** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MBA** | **Vinyl Wall Base/Mastic- Gray** | **Front General Ministry Office** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MBB** | **Vinyl Wall Base/Mastic- Black** | **Faculty Bathroom** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MBC** | **Vinyl Wall Base/Mastic- Brown** | **Supply Room** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MMA** | **Fire Door** | **Boiler Room** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by MEC in 2012*** |
| **MFC** | **12”x12” Floor Tile/Mastic- Brown w/Tan & White Marks** | **Room 102** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by TNC in 2018*** |
| **MFD** | **Sheet Flooring- Brown Wood Pattern** | **Room 105** | **ND** | **ND** |  | **ASSUMED- Preventive Measures… Continue O&M****Material Identified by TNC in 2018** |
| **MBD** | **4” Baseboard/Mastic- Brown** | **Office Area, Room 105** | **ND** | **ND** |  | ***ASSUMED- Preventive Measures… Continue O&M******Material Identified by TNC in 2018*** |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |

 **\*\*\* Material Condition\*\*\***

**(ND)- Not Damaged (D)- Damaged (SD)- Significantly Damaged**

**The 6-month inspection *must* be performed and this form(s) completed by your AHERA-trained employee. Form(s) will be completed no later than March 30th and September 30th of each calendar year. The completed inspection form(s) should then be inserted into your Asbestos Management Plan. A copy of the completed form must also be sent to the Diocesan Property Management Office, attention Brian Heinkel, for insertion into our copy of your Asbestos Management Plan. NOTE:** If the status of the ACBM has changed, then photograph the area and record the photograph number in the space provided. Notify the Asbestos Program Manager immediately concerning any changes.